**Assignment-3**

**LED BLINKING CODE**

import RPi.GPIO as GP

from time importsleep

GP.setwarnings(False)

GP.setmode(GP.BOAR

D)

GP.setup(8,GP.OUT,init

ial=GP.LOW)

while True: #infinite loop

GP.output(8, GPIO.HIGH)

# Turn on print("The LED

is ON")

sleep(2) # Sleep for 2 second

GP.output(8, GPIO.LOW) # Turn off

print("The LED is OFF")sleep(2)

# Sleep for 2 second

**TRAFFIC LIGHTRASBERRY**

**PYTHON CODE**

From gpiozero import LED

From time import sleep

Red= LED(17) #pin numbers connected to Led’s

Aster=(22)

Green=(27)

While True:

Red.on() #RED light

Print(“Red light is ON”)

For I in range(100,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Red.off()

Aster.on() # ASTER light

Print(“Yellow light is ON”)

for I in range(5,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Aster.off()

Green.on #GREEN light

Print(“Green light is ON”)

For I in range(30,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Green.off()